<Description>
C8
Ferrite/Ceramic Magnet
source: https://www.eclipsemagnetics.com/site/assets/files/19602/ferrite_ceramic_datasheet.pdf


<Electric resistivity> at 20*C, (Ohm*m)
100


<Relative permeability>
1.07


<Coercivity> (A/m)   % nominal


<Remanence flux density> (T)    % nominal
0.385

<Intrinsic coercivity> (A/m)
242000


<Temperature coefficient of remanence flux density> (%/deg.C)
-0.2


<Temperature coefficient of intrinsic coercivity> (%/deg.C)
0.27


<Mass Density> (kg/m^3)
5000