<Description>
Recoma 25
SmCo5
Recoma(R) Sintered Samarium Cobalt Magnet
source: http://www.arnoldmagnetics.com/en-us/Products/RECOMA-SmCo-Magnets-en


<Electric resistivity> at 20*C, (Ohm*m)
55e-08


<Relative permeability>



<Coercivity> (A/m)
775000


<Remanence flux density> (T)
1.00


<Intrinsic coercivity> (A/m)
2000000


<Temperature coefficient of remanence flux density> (%/deg.C)
-0.05


<Temperature coefficient of intrinsic coercivity> (%/deg.C)
-0.24


<Mass Density> (kg/m^3)
8400