<Description>
Recoma 33E
Sm2Co17
Recoma(R) Sintered Samarium Cobalt Magnet
source: http://www.arnoldmagnetics.com/en-us/Products/RECOMA-SmCo-Magnets-en


<Electric resistivity> at 20*C, (Ohm*m)
90e-08


<Relative permeability>



<Coercivity> (A/m)
865000


<Remanence flux density> (T)
1.16


<Intrinsic coercivity> (A/m)
2100000


<Temperature coefficient of remanence flux density> (%/deg.C)
-0.035


<Temperature coefficient of intrinsic coercivity> (%/deg.C)
-0.25


<Mass Density> (kg/m^3)
8300