<Description>
N48SH
Neodymium Permanent Magnet
source: http://www.arnoldmagnetics.com/en-us/Products/Neodymium-Magnets


<Electric resistivity> at 20*C, (Ohm*m)
1.3e-06


<Relative permeability>



<Coercivity> (A/m)   % nominal
1039000


<Remanence flux density> (T)    % nominal
1.390

<Intrinsic coercivity> (A/m)
1512000


<Temperature coefficient of remanence flux density> (%/deg.C)
-0.12


<Temperature coefficient of intrinsic coercivity> (%/deg.C)
-0.57

<Mass Density> (kg/m^3)
7600